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ALEX ONE
Main description
Classic Alex towel rail enriched by the built-in One electric heating element. The heating element hidden in the Alex’s collector blends invisibly with its shape – without the need for an additional, external electric device. One is a practical and easy to use heating element which does not dominate the Alex radiator with its form. The curved tube C and the space between the towel rail’s sections allow easy hanging of the fabric to dry. 
Key points
· Classic design of the radiator 
· Easy hanging of the fabric to dry thanks to the curved tube C and the space between the towel rail’s sections
· Functional built-in One electric heating element
Features and benefits of the Alex radiator
· Highest quality low carbon steel ensuring product longevity
· Oxsilan® passive rust protection process
· High quality double layer powder coating
· 8 years warranty for water tightness and paint coating
· Increased resistance to chemicals, temperature variations and mechanical damage
· Easy cleaning and maintenance
· Easy installation (solid wall fixing kit included)
· Made to EN 10305-5
Features and benefits of the One heating element
· Two operation modes: heating and drying 
· TIMER function (automatically switches off the device after 2 hours) 
· Ultra-low power consumption in standby mode (< 0,5 W) 
· Device settings are remembered in case of electricity cut-off, which makes it possible to work with external timers or intelligent building systems 
· Option of adding extra functions by means of the built-in infrared link
· Protection against operation in dry conditions and double protection against radiator overheating 
· Frost protection (ANTIFREEZE)

Specifications
	Height (mm): 		
	1580

	Width (mm): 		
	500

	Depth (mm): 		
	130

	Colour: 			
	Modern Grey

	Heat output (W): 		
	800

	Heat output (BTUs):
	2730

	Connection type:	
	E8

	Connection spacing (mm):
	N/A

	Wall to centre of inlet (mm):	
	N/A

	Operating pressure (MPa):	
	1

	Maximum operating temperature (°C):
	60

	Material:
	Carbon steel

	Surface finish:
	Powder coating

	Weight (kg):
	22,99



Connection diagram
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