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JADE
Main description
The classic towel rail. Wide gaps between profile sections make it a functional dryer. Jade can become an inconspicuous decorative feature of each room.
Key points
· Modern design 
· Functional and light towel rail
· Easy access to clothes and towels
Features and benefits
· Highest quality low carbon steel ensuring product longevity
· Every rail 100% leak tested
· Hand polished surface ensuring state-of-the-art galvanic coating
· Great towel hanging capability
· Easy installation (solid wall fixing kit included)
· Easy cleaning and maintenance
· Made to EN 10305-5
· Bleed valve included
Specifications
	Height (mm): 		
	1149

	Width (mm): 		
	400

	Depth (mm): 		
	61

	Colour: 			
	Galvanic Old Copper

	Heat output (W): 		
	252

	Heat output (BTUs):
	860

	Connection type:	
	SX

	Connection spacing:
	364

	Wall to centre of inlet (mm):	
	52-72

	Operating pressure (MPa):	
	1

	Maximum operating temperature (°C):
	95

	Material:
	Carbon steel

	Surface finish:
	Galvanic coating

	Weight (kg):
	6.89
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