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Swale
Main description
New technologies allow radiator designers to introduce new and uncommon forms. Original design, highest quality and functionality make Swale a great choice not only for bathrooms, but also for other spaces in modern interiors.

Key points
· Unique asymmetric form 
· Original and functional decorative element
· Ultimate minimalism and practical value
Features and benefits
· Highest quality low carbon steel ensuring product longevity
· Every rail 100% leak tested
· Oxsilan® passive rust protection process
· Great towel hanging capability
· High quality double layer powder coating
· Up to 8 Year Guarantee
· Increased resistance to chemicals, temperature variations and mechanical damage
· Easy installation (solid wall fixing kit included)
· Easy cleaning and maintenance
· Made to EN 10305-5
· Bleed valve included
Specifications
	Height (mm): 		
	1200

	Width (mm): 		
	465

	Depth (mm): 		
	32

	Colour: 			
	Metallic Black

	Heat output (W): 		
	757

	Heat output (BTUs):
	[bookmark: _GoBack]2583

	Connection type:	
	YP

	Connection spacing:
	50

	Wall to centre of inlet (mm):	
	67-75

	Operating pressure (MPa):	
	1

	Maximum operating temperature (°C):
	95

	Material:
	Carbon steel

	Surface finish:
	Powder coating

	Weight (kg):
	13
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